|  |
| --- |
| **DWS safes - DWS-F** |
| **Certified burglary protection according to EN 1143-1 Grad IV****DWS-F: Certified fire protection according to EN 15659 LFS 60P** |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Type** | **Dimensions ext. (mm)** | **Dimensions int. (mm)** | **Weight/Vol** | **Shelves** |
|  | **H** | **L** | **P** | **H** | **L** | **P** | **Kg/litres** |  |
| Certified burglary protection according to EN 1143-1 Grad IV |
| DWS 0849 | 848 | 645 | 565 | 695 | 495 | 320 | 635/110 | 1 |
| DWS 0850 | 848 | 810 | 725 | 695 | 660 | 480 | 875/220 | 1 |
| DWS 1000 | 1003 | 810 | 725 | 850 | 660 | 480 | 1030/269 | 2 |
| DWS 1200 | 1193 | 810 | 725 | 1040 | 660 | 480 | 1150/329 | 2 |
| DWS 1600 | 1538 | 810 | 725 | 1385 | 660 | 480 | 1405/439 | 3 |
| DWS 1901 | 1883 | 810 | 725 | 1730 | 660 | 480 | 1680/548 | 4 |
| DWS 1903 | 1883 | 1110 | 725 | 1730 | 960 | 480 | 2090/797 | 4 |
| DWS 1902 | 1883 | 1110 | 725 | 1730 | 960 | 480 | 2130/797 | 4 |
| DWS 1904 | 1883 | 1415 | 725 | 1730 | 1265 | 480 | 2550/1050 | 4 |
| Certified burglary protection according to EN 1143-1 Grad IVDWS-F: Certified fire protection according to EN 15659 LFS 60P |
| DWS-F 0850 | 848 | 810 | 725 | 695 | 660 | 480 | 875/220 | 1 |
| DWS-F 1000 | 1003 | 810 | 725 | 850 | 660 | 480 | 1030/269 | 2 |
| DWS-F 1200 | 1193 | 810 | 725 | 1040 | 660 | 480 | 1150/329 | 2 |
| DWS-F 1600 | 1538 | 810 | 725 | 1385 | 660 | 480 | 1405/439 | 3 |
| DWS-F 1901 | 1883 | 810 | 725 | 1730 | 660 | 480 | 1680/548 | 4 |
| DWS-F 1903 | 1883 | 1110 | 725 | 1730 | 960 | 480 | 2090/797 | 4 |
| Profondeur : + 60 mm pour charnières |

****

*It simply has no weak points*

**Technical data :**

- Fire test 60 minutes

 for paper (models DWS-F)

- Solid locking on all sides

- Multi-wall construction

- All sides reinforced with material

 extremely resistant

- Sensitive points protected by

 additional reinforcements

- Shielding of the locking system

- Locking of the lock and bolts in

 test case of burglary by means of an informer lock

- Alarm pre-equipment

- Device for floor and wall mounting

**Standard finish :**

- Electronic locks (Paxos)

- Removable shelves

- Two-tone grey RAL 7035 and RAL 7045

- Door pivots: right or left

 DWS 1902 and DWS 1904 with two doors

**Options :**

- Other locks on request

 (two mandatory locks at

 From Class IV onwards)

- From model 1600 upwards: available

 with bank compartments

- Available with anti-drilling by

 diamond crown

- Available in modular version

 (DWS models from size 1000 upwards)

- Special colours

- Interior fittings according to

 the price list

**TECHNO SAFE Coffres-forts**

Avenue Industrielle 5, 1227 Carouge

+41 22 343 21 14

info@technosafe.ch / www.technosafe.ch

DWS 1200