
|  |
| --- |
| **Safes Series D** |
| **Certified burglary protection according to EN 1143-1 Grad IV** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Type** | **Dimensions ext. (mm)** | | | **Dimensions int. (mm)** | | | | **Weight/Vol** | | **Shelves** |
|  | **H** | **L** | **P** | **H** | **L** | | **P** | **Kg/litres** | |  |
| Certified burglary protection according to EN 1143-1 Grad IV | | | | | | | | | | |
| D94/40 | 1160 | 610 | 620 | 940 | 402 | 335 | | 541/144 | 1 | |
| D104/40 | 1260 | 610 | 620 | 1040 | 402 | 335 | | 579/158 | 1 | |
| D124/40 | 1460 | 610 | 620 | 1240 | 402 | 335 | | 655/188 | 2 | |
| D144/40 | 1660 | 610 | 620 | 1440 | 402 | 335 | | 730/218 | 2 | |
| D94/60 | 1160 | 810 | 730 | 940 | 602 | 445 | | 765/277 | 1 | |
| D104/60 | 1260 | 810 | 730 | 1040 | 602 | 445 | | 817/306 | 1 | |
| D124/60 | 1460 | 810 | 730 | 1240 | 602 | 445 | | 921/363 | 2 | |
| D144/60 | 1660 | 810 | 730 | 1440 | 602 | 445 | | 1025/420 | 2 | |
| D164/60 | 1860 | 810 | 730 | 1640 | 602 | 445 | | 1129/477 | 3 | |
| D184/60 | 2060 | 810 | 730 | 1840 | 602 | 445 | | 1233/534 | 4 | |
| D94/75 | 1160 | 960 | 790 | 940 | 752 | 505 | | 936/388 | 1 | |
| D104/75 | 1260 | 960 | 790 | 1040 | 752 | 505 | | 999/428 | 1 | |
| D124/75 | 1460 | 960 | 790 | 1240 | 752 | 505 | | 1124/508 | 2 | |
| D144/75 | 1660 | 960 | 790 | 1440 | 752 | 505 | | 1250/588 | 2 | |
| D164/75 | 1860 | 960 | 790 | 1640 | 752 | 505 | | 1375/668 | 3 | |
| D184/75 | 2060 | 960 | 790 | 1840 | 752 | 505 | | 1500/748 | 4 | |
| D194/75 | 2160 | 960 | 790 | 1940 | 752 | 505 | | 1563/788 | 4 | |
| D164/100 | 1860 | 1210 | 790 | 1640 | 1002 | 505 | | 1762/879 | 3 | |
| D184/100 | 2060 | 1210 | 790 | 1840 | 1002 | 505 | | 1923/984 | 4 | |



**TECHNO SAFE Coffres-forts**

Avenue Industrielle 5, 1227 Carouge

+41 22 343 21 14

[info@technosafe.ch](mailto:info@technosafe.ch) / www.technosafe.ch

*Made in Switzerland*

**Technical data :**

- Innovative shielding

- Solid locking on all sides

- Lock and bolts are blocked in the event of a break-in attempt

By informer lock

- Electronic lock with Paxos redundancy

- Removable shelves

- Pre-equipment for alarm

- Colour: Light grey RAL 7035

- Door pivots on the right

- Device for fixing to the floor

- Made in Switzerland

**Options :**

- Other locks on request

- Two locks compulsory from Class IV onwards

- Special colours